List
- [[BMW X5|BMW X5]]
- [[Nissan Altima]]

  

**Sources**
- [NHTSA](https://www.nhtsa.gov/ratings) - National Highway Traffic Safety Administration
- [JD Power](https://www.jdpower.com/cars/ratings) and [2024 Most Reliable Vehicles - U.S. Dependability Study](https://www.jdpower.com/business/press-releases/2024-us-vehicle-dependability-study-vds)
- [2024 JD Power report.pdf](app://obsidian.md/2024%20JD%20Power%20report.pdf)
- [IIHS](https://www.iihs.org/ratings) - Insurance Institute for Highway Safety
- [Understanding car safety ratings](https://www.chase.com/personal/auto/education/buying/car-safety-ratings)

### Car maintenance
- Battery maintenance tips  
    For proper alternator functioning, turn on the car, the battery will get charging and will show 14.2V to 14.7V on multimeter. If it’s above 14.7V, then alternator is overcharging the battery.  
    If voltage is below 14.2V, say 13V then the alternator isn’t charging the battery properly. It’ll still charge it but you’ll burn more fuel for the same charge.
    [how-to-install-a-top-post-car-battery](https://www.autozone.com/diy/battery/how-to-install-a-top-post-car-battery)  
    [how-to-check-a-car-battery](https://axleaddict.com/auto-repair/check-a-car-battery)
- **Tire maintenance tips**
	- [Tire Care Essentials | U.S. Tire Manufacturers Association (ustires.org)](https://www.ustires.org/tire-care-essentials)
	- **Inflation**:
		- Check tire pressure when vehicle is at rest in the morning at least once a month
		- Impact of temperature: For every 10 degrees F change in ambient temperature, tire pressure will change by approximately 1 PSI.
	- **Rotation and wheel balancing**:
		- USTMA recommends every 5,000 to 8,000 miles
		- Have your tires balanced every time you change or rotate your tires or when you install a new set of wheels.
		- Nissan manual says Tires should be rotated every 5,000 miles (8,000 km)

